{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["凯尔乐"],"not_rendered":{"images":5},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"凯尔乐","index":0,"n_rows":113,"n_cols":5,"rows_kept":113,"merged":[[0,1,0,3],[0,4,0,5],[1,1,1,3],[1,4,1,5],[2,1,2,3],[2,4,2,5],[3,1,3,3],[3,4,3,5],[4,1,4,3],[4,4,4,5],[5,1,5,3],[5,4,5,5],[6,1,6,3],[6,4,6,5],[7,1,7,3],[7,4,7,5],[8,1,8,3],[8,4,8,5],[9,1,9,3],[9,4,9,5],[10,1,10,3],[10,4,10,5],[17,1,17,3],[17,4,17,5],[18,1,18,3],[18,4,18,5],[19,1,19,3],[19,4,19,5],[20,1,20,3],[20,4,20,5],[21,1,21,3],[21,4,21,5],[22,1,22,3],[22,4,22,5],[23,1,23,3],[23,4,23,5],[24,1,24,3],[24,4,24,5],[25,1,25,3],[25,4,25,5],[26,1,26,3],[26,4,26,5],[27,1,27,3],[27,4,27,5],[44,1,44,3],[44,4,44,5],[45,1,45,3],[45,4,45,5],[46,1,46,3],[46,4,46,5],[47,1,47,3],[47,4,47,5],[48,1,48,3],[48,4,48,5],[49,1,49,3],[49,4,49,5],[50,1,50,3],[50,4,50,5],[51,1,51,3],[51,4,51,5],[52,1,52,3],[52,4,52,5],[53,1,53,3],[53,4,53,5],[54,1,54,3],[54,4,54,5],[68,1,68,3],[68,4,68,5],[69,1,69,3],[69,4,69,5],[70,1,70,3],[70,4,70,5],[71,1,71,3],[71,4,71,5],[72,1,72,3],[72,4,72,5],[73,1,73,3],[73,4,73,5],[74,1,74,3],[74,4,74,5],[75,1,75,3],[75,4,75,5],[76,1,76,3],[76,4,76,5],[77,1,77,3],[77,4,77,5],[78,1,78,3],[78,4,78,5],[92,1,92,3],[92,4,92,5],[93,1,93,3],[93,4,93,5],[94,1,94,3],[94,4,94,5],[95,1,95,3],[95,4,95,5],[96,1,96,3],[96,4,96,5],[97,1,97,3],[97,4,97,5],[98,1,98,3],[98,4,98,5],[99,1,99,3],[99,4,99,5],[100,1,100,3],[100,4,100,5],[101,1,101,3],[101,4,101,5],[102,1,102,3],[102,4,102,5]],"flags":["formulas_cached_only"]}
[null,"产品名称",null,null,"电瓶肩背式吸尘器"]
[null,"产品型号",null,null,"KEB 0706B48"]
[null,"电压",null,null,"DC48"]
[null,"流量 m3/h",null,null,234]
[null,"功率 W",null,null,700]
[null,"风压 kpa",null,null,24.7]
[null,"容量 L",null,null,6]
[null,"电瓶容量 AH",null,null,"14(锂电）"]
[null,"过滤精度 μm",null,null,0.2]
[null,"尺寸 cm",null,null,"直径270*高度570"]
[null,"工作时间 min",null,null,40]
[null,"特点及应用："]
[null,"电瓶肩背式吸尘器是在肩背式吸尘器的基础上研发的一款，对无电源区域一种清洁的新方式，如电影院、巴士、机舱、高铁等。体积小方便携带，360度转身灵活，移动方便快捷，吸尘效果好，经济实惠。"]
[]
[]
[]
[]
[null,"产品名称",null,null,"电瓶式工业吸尘器"]
[null,"产品型号",null,null,"KEB 0715B48"]
[null,"电压",null,null,"DC48"]
[null,"流量 m3/h",null,null,234]
[null,"功率 W",null,null,700]
[null,"风压 kpa",null,null,24.7]
[null,"容量 L",null,null,15]
[null,"电瓶容量 AH",null,null,30]
[null,"过滤精度 μm",null,null,0.2]
[null,"尺寸 cm",null,null,"55*38*100"]
[null,"工作时间 H",null,null,2]
[null,"产品特点："]
[null,"1.采用交直流干湿两用型电机，可吸尘、吸水同时完成给您的工作带来便利。"]
[null,"2.电机单独启动，可以有限延长使用时间，工作效率高。"]
[null,"3.倾倒式集尘桶，可加装垃圾袋更加方便清倒垃圾，避免二次污染。"]
[null,"4.电池30AH,工作时间自由掌控。"]
[null,"5.不锈钢金属材料，坚固耐用、耐磨、不易划伤。"]
[null,"6.配备高效过滤器，有效延长工作时间，过滤精度，0.2μm，排出的空气可达99.9%。"]
[null,"7.无电线缠绕，可以在复杂的车间自由穿梭，工作效率倍增。"]
[null,"8.满足一般的清洁工作时间需求。配置高品质充电器，充电：8-10小时即可充满。"]
[null,"9.应用场所：大型工厂、广场、郊外、冶金、煤矿、环卫设备配套使用、地下车库等。"]
[]
[]
[]
[]
[]
[]
[null,"产品名称",null,null,"电瓶式工业吸尘器"]
[null,"产品型号",null,null,"KEB 1060B24"]
[null,"电压",null,null,"DC24"]
[null,"流量 m3/h",null,null,234]
[null,"功率 W",null,null,1000]
[null,"风压 kpa",null,null,24.7]
[null,"容量 L",null,null,60]
[null,"电瓶容量 AH",null,null,120]
[null,"过滤精度 μm",null,null,0.2]
[null,"尺寸 cm",null,null,"75*63*109"]
[null,"工作时间 H",null,null,4]
[null,"产品特点："]
[null,"1.采用交直流干湿两用型电机，可吸尘、吸水同时完成给您的工作带来便利。"]
[null,"2.电机单独启动，可以有限延长使用时间，工作效率高。"]
[null,"3.倾倒式集尘桶，可加装垃圾袋更加方便清倒垃圾，避免二次污染。"]
[null,"4.电池30AH,工作时间自由掌控。"]
[null,"5.不锈钢金属材料，坚固耐用、耐磨、不易划伤。"]
[null,"6.配备高效过滤器，有效延长工作时间，过滤精度，0.2μm，排出的空气可达99.9%。"]
[null,"7.无电线缠绕，可以在复杂的车间自由穿梭，工作效率倍增。"]
[null,"8.满足一般的清洁工作时间需求。配置高品质充电器，充电：8-10小时即可充满。"]
[null,"9.应用场所：大型工厂、广场、郊外、冶金、煤矿、环卫设备配套使用、地下车库等。"]
[]
[]
[]
[null,"产品名称",null,null,"电瓶式工业吸尘器"]
[null,"产品型号",null,null,"KEB 1580B24"]
[null,"电压",null,null,"DC24"]
[null,"流量 m3/h",null,null,351]
[null,"功率 W",null,null,1500]
[null,"风压 kpa",null,null,37]
[null,"容量 L",null,null,80]
[null,"电瓶容量 AH",null,null,120]
[null,"过滤精度 μm",null,null,0.2]
[null,"尺寸 cm",null,null,"80*50*1130"]
[null,"工作时间 H",null,null,"4-5"]
[null,"产品特点："]
[null,"1.采用交直流干湿两用型电机，可吸尘、吸水同时完成给您的工作带来便利。"]
[null,"2.电机单独启动，可以有限延长使用时间，工作效率高。"]
[null,"3.倾倒式集尘桶，可加装垃圾袋更加方便清倒垃圾，避免二次污染。"]
[null,"4.电池30AH,工作时间自由掌控。"]
[null,"5.不锈钢金属材料，坚固耐用、耐磨、不易划伤。"]
[null,"6.配备高效过滤器，有效延长工作时间，过滤精度，0.2μm，排出的空气可达99.9%。"]
[null,"7.无电线缠绕，可以在复杂的车间自由穿梭，工作效率倍增。"]
[null,"8.满足一般的清洁工作时间需求。配置高品质充电器，充电：8-10小时即可充满。"]
[null,"9.应用场所：大型工厂、广场、郊外、冶金、煤矿、环卫设备配套使用、地下车库等。"]
[]
[]
[]
[null,"产品名称",null,null,"电瓶式带推吸功能工业吸尘器"]
[null,"产品型号",null,null,"KEP 1580B24"]
[null,"电压",null,null,"DC24"]
[null,"流量 m3/h",null,null,351]
[null,"功率 W",null,null,1500]
[null,"风压 kpa",null,null,37]
[null,"容量 L",null,null,80]
[null,"电瓶容量 AH",null,null,120]
[null,"过滤精度 μm",null,null,0.2]
[null,"尺寸 cm",null,null,"80*50*1130"]
[null,"工作时间 H",null,null,"4-5"]
[null,"产品特点："]
[null,"1.采用交直流干湿两用型电机，可吸尘、吸水同时完成给您的工作带来便利。"]
[null,"2.电机单独启动，可以有限延长使用时间，工作效率高。"]
[null,"3.倾倒式集尘桶，可加装垃圾袋更加方便清倒垃圾，避免二次污染。"]
[null,"4.电池30AH,工作时间自由掌控。"]
[null,"5.不锈钢金属材料，坚固耐用、耐磨、不易划伤。"]
[null,"6.配备高效过滤器，有效延长工作时间，过滤精度，0.2μm，排出的空气可达99.9%。"]
[null,"7.无电线缠绕，可以在复杂的车间自由穿梭，工作效率倍增。"]
[null,"8.满足一般的清洁工作时间需求。配置高品质充电器，充电：8-10小时即可充满。"]
[null,"9.应用场所：大型工厂、广场、郊外、冶金、煤矿、环卫设备配套使用、地下车库等。"]